Network
Voice
SIP Proxy
Dial Plan
System
Technical Support
Basic Information
Phone Model:
MAC Address:
OEM Tag:
Version No.:
Network Settings
Connection Type: |
IP Address: |
Subnet Mask: |
Default Gateway: |
PPPoE User ID: |
PPPoE User PIN: |
Automatically get DNS server IP
Use following DNS server IP
Primary DNS: |
Secondary DNS: |
Layer 3 QoS: | (Diff-Serv or Precedence value)
Layer 2 QoS: | 802.1Q VLAN Tag
| 802.1p Priority Value
Voice Codec Settings
Preferred Voice Codec: | Codec 1: Frames per TX 1:
(In listed order) | Codec 2: Frames per TX 2:
| Codec 3: Frames per TX 3:
| Codec 4: Frames per TX 4:
| Codec 5: Frames per TX 5:
| Codec 6: Frames per TX 6:
| Codec 7: Frames per TX 7:
( Frames Per TX Range: PCMU, PCMA, iLBC and Speex between 1 and 3; G.726-32, GSM 6.10 and G.729 between 1 and 6 )
iLBC Frame Size: | 20ms 30ms
Speex Rate: |
Voice Activity Detection (VAD): | No Yes
Automatic Gain Control (AGC): | No Yes
Acoustic Echo Cancellation (AEC): | No Yes
Basic SIP Proxy Settings
SIP Registration: | No Yes
SIP Server: | (IP or URI)
SIP Server Port: | (Default 5060)
SIP Domain: |
SIP Server As Outbound Proxy: | No Yes
Use DNS SRV: | No Yes
SIP User ID: |
SIP Authentication ID: |
SIP Authentication PIN: |
User Name: | (Optional, e.g., Woody Allen)
Advanced SIP Proxy Settings
Local SIP Port: | (Default 5060)
Local RTP Port: | (Between 1024 and 65535, default 6000)
Register Expiration: | (In seconds, default 60s)
Keep Alive Interval: | (In seconds, default 20s)
Send DTMF: |
DTMF Payload Type: | (Between 96 and 127, default 101)
G.726-32 Payload Type: | (Between 96 and 127, default 111)
iLBC Payload Type: | (Between 96 and 127, default 98)
Speex Payload Type: | (Between 96 and 127, default 110)
Message Service Number: |
Support PRACK(100rel, RFC3262): | No Yes
Subscribe for MWI: | No Yes
Proxy Require: |
NAT Traversal: |
NAT IP: |
STUN Server: | (IP or URI)
STUN Server Port: | (Default 3478)
Dial Plan Settings
Forward-to Number: |
Forward Unconditionally: | No Yes
Forward When Busy: | No Yes
Forward When No Answer: | No Yes
No Answer Timeout: | (In seconds, default 60s)
Auto Answer: | No Yes
Call Waiting: | No Yes
Dial Prefix: | (It's added to each dialed number)
Hot Line Number: | (Number dialed when handset up)
Use Digit Maps: | No Yes
Digit Maps Timeout: | (In seconds, default 5s)
Use "#" To Call: | No Yes
System Settings
Administration Password: | (Password to enter this web)
Syslog IP: |
Handset Input (0-7): |
Handset Output (0-31): |
Speaker Output (0-31): |
Ring Volume (10-31): |
Auto Provisioning Server: | (IP or URI)
Auto Provisioning Port: | (Default 80)
Auto Provisioning Interval: | (In minutes, maximum 65535 minutes)
SNTP Server: | (IP or URI, e.g, time.windows.com)
Time Zone: |
Automatically Adjust Clock for Daylight Saving Changes: | No Yes
Technical Support
PalmMicro is trying to offer you IP phone with the highest quality. If you have any inquiries about the product, please contact us or login on our technical support web site for help. Go to PalmMicro