Network
Voice
IAX2 Protocol
Dial Plan
System
Technical Support
Basic Information
Phone Model:
MAC Address:
OEM Tag:
Version No.:
Network Settings
Connection Type: |
IP Address: |
Subnet Mask: |
Default Gateway: |
PPPoE User ID: |
PPPoE User PIN: |
Automatically get DNS server IP
Use following DNS server IP
Primary DNS: |
Secondary DNS: |
Layer 3 QoS: | (Diff-Serv or Precedence value)
Layer 2 QoS: | 802.1Q VLAN Tag
| 802.1p Priority Value
Voice Codec Settings
Preferred Voice Codec: | Codec 1: Frames per TX 1:
(In listed order) | Codec 2: Frames per TX 2:
| Codec 3: Frames per TX 3:
| Codec 4: Frames per TX 4:
| Codec 5: Frames per TX 5:
| Codec 6: Frames per TX 6:
| Codec 7: Frames per TX 7:
( Frames Per TX Range: PCMU, PCMA, G.726-32, G.729, between 1 and 7; GSM 6.10, Speex, iLBC-20ms, between 1 and 4; iLBC-30ms, between 1 and 3 )
iLBC Frame Size: | 20ms 30ms
Speex Rate: |
Voice Activity Detection (VAD): | No Yes
Automatic Gain Control (AGC): | No Yes
Acoustic Echo Cancellation (AEC): | No Yes
IAX2 Protocol Settings
IAX2 Registration: | No Yes
IAX2 Server: | (IP or URI)
IAX2 Server Port: | (Default 4569)
IAX2 User ID: |
IAX2 Authentication ID: |
IAX2 Authentication PIN: |
User Name: | (Optional, e.g., Woody Allen)
Local IAX2 Port: | (Default 4569)
Register Expiration: | (In seconds, default 60s)
Message Service Number: |
Use Server's Dial Plan: | No Yes
Dial Plan Settings
Forward-to Number: |
Forward Unconditionally: | No Yes
Forward When Busy: | No Yes
Forward When No Answer: | No Yes
No Answer Timeout: | (In seconds, default 60s)
Auto Answer: | No Yes
Call Waiting: | No Yes
Dial Prefix: | (It's added to each dialed number)
Hot Line Number: | (Number dialed when handset up)
Use Digit Maps: | No Yes
Digit Maps Timeout: | (In seconds, default 5s)
Use "#" To Call: | No Yes
System Settings
Administration Password: | (Password to enter this web)
Syslog IP: |
Handset Input (0-7): |
Handset Output (0-31): |
Speaker Output (0-31): |
Auto Provisioning Server: | (IP or URI)
Auto Provisioning Port: | (Default 80)
Auto Provisioning Interval: | (In minutes, maximum 65535 minutes)
SNTP Server: | (IP or URI, e.g, time.windows.com)
Time Zone: |
Automatically Adjust Clock for Daylight Saving Changes: | No Yes
Technical Support
PalmMicro is trying to offer you IP phone with the highest quality. If you have any inquiries about the product, please contact us or login on our technical support web site for help. Go to PalmMicro