Network
Voice
SIP Proxy
Dial Plan
System
Technical Support
Basic Information
Phone Model: MTA7308-SL
MAC Address:
Version No.:
Network Settings
Connection Type: |
IP Address: |
Subnet Mask: |
Default Gateway: |
PPPoE User ID: |
PPPoE User PIN: |
Automatically get DNS server IP
Use following DNS server IP
Primary DNS: |
Secondary DNS: |
Layer 3 QoS: | (Diff-Serv or Precedence value)
Layer 2 QoS: | 802.1Q VLAN Tag
| 802.1p Priority Value
Voice Codec Settings
Preferred Voice Codec: | Codec 1: Frames per TX 1:
(In listed order) | Codec 2: Frames per TX 2:
| Codec 3: Frames per TX 3:
| Codec 4: Frames per TX 4:
| Codec 5: Frames per TX 5:
| Codec 6: Frames per TX 6:
| Codec 7: Frames per TX 7:
( Frames Per TX Range: PCMU, PCMA, G.726-32, G.729, between 1 and 7; GSM 6.10, Speex, iLBC-20ms, between 1 and 4; iLBC-30ms, between 1 and 3 )
iLBC Frame Size: | 20ms 30ms
Speex Rate: |
Voice Activity Detection (VAD): | No Yes
Automatic Gain Control (AGC): | No Yes
Acoustic Echo Cancellation (AEC): | No Yes
Basic SIP Proxy Settings
SIP Registration: | No Yes
SIP Server: | (IP or URI)
SIP Server Port: | (Default 5060)
SIP Domain: |
SIP Server As Outbound Proxy: | No Yes
Use DNS SRV: | No Yes
SIP User ID: |
SIP Authentication ID: |
SIP Authentication PIN: |
User Name: | (Optional, e.g., Woody Allen)
Advanced SIP Proxy Settings
Local SIP Port: | (Default 5060)
Local RTP Port: | (Between 1024 and 65535, default 6000)
Register Expiration: | (In seconds, default 60s)
Keep Alive Interval: | (In seconds, default 20s)
Send DTMF: |
DTMF Payload Type: | (Between 96 and 127, default 101)
G.726-32 Payload Type: | (Between 96 and 127, default 111)
iLBC Payload Type: | (Between 96 and 127, default 98)
Speex Payload Type: | (Between 96 and 127, default 110)
Message Service Number: |
Support PRACK(100rel, RFC3262): | No Yes
Subscribe for MWI: | No Yes
Proxy Require: |
NAT Traversal: |
NAT IP: |
STUN Server: | (IP or URI)
STUN Server Port: | (Default 3478)
Dial Plan Settings
Forward-to Number: |
Forward Unconditionally: | No Yes
Forward When Busy: | No Yes
Forward When No Answer: | No Yes
No Answer Timeout: | (In seconds, default 60s)
Auto Answer: | No Yes
Call Waiting: | No Yes
Dial Prefix: | (It's added to each dialed number)
Hot Line Number: | (Number dialed when handset up)
Use Digit Maps: | No Yes
Digit Maps Timeout: | (In seconds, default 5s)
Use "#" To Call: | No Yes
System Settings
Administration User Name: | (Username to enter this web)
Administration Password: | (Password to enter this web)
Syslog IP: |
Handset Input (0-7): |
Handset Output (0-31): |
Speaker Output (0-31): |
Ring Volume (10-31): |
Auto-provisioning Interval: | (In minutes, maximum 65535 minutes)
SNTP Server: | (IP or URI, e.g, time.windows.com)
Time Zone: |
Automatically Adjust Clock for Daylight Saving Changes: | No Yes
Technical Support
If you have any inquiries about the product, please contact us or login on our technical support web site for help. Go to InnoMedia